BOOTER
------
release January, 22, 2015
version 1.0.3

About:
Booter scans every drive (in range 8 - 30) connected to Commodore 128 for "BOOT.CFG" file. If is found reads its data and execute action by data.
BOOT.CFG file can be placed on selected drive by user in default partition. File can be also on other drives, but scan begins at drive 8 so first found BOOT.CFG file in this order will be executed. BOOT.CFG file is bootsector independent.

BOOT.CFG file data decription:
program type: BASIC, ML, DATA
drive: 8 - 30
filename: user defined
actions by type:
ML executes code starting at load address of selected file
BASIC - is possible to define versions 2.0, 3.5, 7.0, 10.0 - load address is always corrected to Commodore 128 native mode ($1C01 / $4001) no matter if specified file is written f.e. in Basic 2.0 (so has start address $0801), after loading performs RUN command
DATA loads any data to specified address, then performs Commodore 128 default booting

BOOT.CFG CREATOR
- simple Basic 7.0 file providing wizard to create BOOT.CFG file

code:		Miro Karkus
thanks to: 	Robert Willie (aka Hydrophilic)
-----------------
(C)2015 MIRKOSOFT